## **Lebanese UniversityLebanese University** الجامعة اللبنانية

**Faculty of Engineering** كلية الهندسة

**Branch III** الفرع الثالث

**Matlab**

**Project**

*Presented to:*  **Dr. Hassan Naim**

*Done by:*

* **Hassan Mohsen - 6295**
* **Dima Azzam - 6302**
* **Yamen Salman - 6412**

Table of Contents:

1. General Concepts
   1. Introduction……………………………………………. page 4
   2. Definitions……………………………………………… page 5
   3. MATLAB Overview…………………………………… page 6
2. Solar Energy
   1. Concept………………………………………………… pages 7-8
   2. Equations of Performance……………………………. page 8→11
   3. Simulation……………………………………………. page 12→20
   4. Analysis………………………………………………. page 21
3. Wind Energy
   1. Concept………………………………………………. pages 22-23
   2. Equations of Performance…………………………... page 23→25
   3. Simulation…………………………………………. page 25→30
   4. Analysis……………………………………………. page 31
4. Conclusion………………………………………………… page 31

5. References………………………………………………… page 32


**1.1 Introduction**

In our quest for a sustainable and efficient energy future, the concept of the smart grid has emerged as a game-changer. The smart grid is a revolutionary electrical infrastructure that leverages advanced technologies to optimize the generation, distribution, and consumption of electricity. It lays the foundation for integrating multiple electricity sources, including solar and wind power, like never before (figure 1-a).




At its core, the smart grid represents a paradigm shift from the traditional one-way power flow model to a two-way, interactive system. It enables a seamless integration of diverse energy sources into the grid, facilitating a more reliable, resilient, and environmentally friendly energy ecosystem.

**Figure 1-a**

**

By intricately aligning the intricate dynamics of solar and wind energy, the smart grid emerges as a pioneering force in the realm of renewable power integration. Leveraging advanced algorithms, real-time monitoring, and predictive analytics, the smart grid enables precise forecasting, efficient generation, and seamless synchronization of solar and wind resources (figure 1-b).

**

**Figure 1-b**

**Figure 1-c**

As the smart grid evolves, it embraces the whispering winds (figure 1-c) and the radiant sun, seamlessly integrating the bountiful energy they offer. Together, solar and wind power are gracefully woven into the fabric of the smart grid, empowering a sustainable energy ecosystem that lights our path towards a greener future.

**1.2 Definitions**

***Power:*** *The rate at which energy is transferred or used in a system.*

***Current:*** *The flow of electric charge through a conductor.*

***Potential:*** *The amount of electrical energy possessed by a charged object due to its position relative to other charged objects.*

***Smart grid:*** *An advanced electricity distribution network that uses digital technologies to optimize the generation, distribution, and consumption of electricity.*

***Efficiency:*** *The ratio of useful output or work produced by a system to the total input or energy provided to the system.*

***Emissivity:*** *The measure of a material's ability to emit thermal radiation.*

***Incident angle:*** *The angle at which a beam of light or radiation strikes a surface*.

***Latitude:*** *refers to the angular distance, measured in degrees, between a specific location on Earth and the equator, indicating whether the location is north or south of the equator.*

***Longitude:*** *refers to the angular distance, also measured in degrees, between a specific location and the Prime Meridian, which runs through Greenwich, London. It indicates whether the location is east or west of the Prime Meridian.*

**1.3- MATLAB overview**

MATLAB is a powerful software tool widely used in various scientific and engineering domains, including the solar and wind energy sectors. Here's an overview of how MATLAB can assist in the analysis, design, and optimization of solar and wind systems:



*Modeling and Simulation:* In solar and wind applications, you can develop mathematical models that represent the behavior of solar panels, wind turbines, and other components. By simulating these models in MATLAB, you can assess the performance, efficiency, and reliability of solar and wind systems under different operating conditions. This helps in the design and optimization of system configurations, control strategies, and energy yield estimation.

*Data Analysis and Visualization:* In the solar and wind domain, you can use MATLAB to process and analyze weather data, such as solar irradiance and wind speed measurements. You can plot and visualize the data to gain insights into the characteristics of the resource, identify patterns, and make informed decisions about system design and operation.

*Control System Design:* MATLAB provides powerful tools for designing and simulating control systems. In the context of solar and wind energy, control systems play a crucial role in maximizing energy capture, optimizing power output, and ensuring grid stability. MATLAB enables the development and testing of control algorithms for solar tracking systems, pitch control in wind turbines, power converters, and grid integration mechanisms. It allows engineers to iterate, refine, and validate control strategies before implementing them in real-world systems

*Deployment and Hardware Integration:* MATLAB supports the deployment of algorithms and models to embedded systems, hardware platforms, and real-time applications. This feature is valuable for implementing control algorithms and monitoring systems in solar and wind installations. It also integrates with hardware devices such as data acquisition systems and programmable logic controllers (PLCs), allowing you to interface with sensors, actuators, and other equipment in the field.

*Optimization and Parameter Estimation:* MATLAB allows engineers to define objective functions and constraints, and then find optimal values for system parameters. For example, you can use it to optimize the design of a solar panel array for maximum energy production or to optimize the rotor design of a wind turbine for enhanced efficiency. Additionally, MATLAB provides tools for parameter estimation, allowing you to calibrate models based on measured data to improve their accuracy.



**Figure 2-a** and **2-b**: Use of matlab in simulative and engineering appliances


**2.1 Concept**

Solar energy is a renewable and environmentally friendly power source that converts sunlight into electricity or thermal energy. It utilizes photovoltaic cells or solar thermal systems. Solar power is abundant, reduces reliance on fossil fuels, and is experiencing significant growth in the global energy transition.

Solar energy works by harnessing the power of sunlight through photovoltaic cells. Photovoltaic (PV) cells, commonly known as solar cells, are made of semiconductor materials, such as silicon. When sunlight hits the PV cells, it excites the electrons in the material, generating an electric current.

The PV cells are typically arranged in solar panels, which are then connected to an inverter. The inverter converts the direct current (DC) produced by the solar panels into alternating current (AC) electricity, which is the type of electricity used in homes and businesses.

The process of converting sunlight into electricity in photovoltaic cells involves the following steps:

1. **Absorption:** The PV cells are designed to absorb photons from sunlight. Photons are particles of light that carry energy.
2. **Electron Excitation:** When photons are absorbed by the semiconductor material in the PV cell, they transfer their energy to the electrons in the material, causing them to become "excited" as shown in figure 3. This energy allows the electrons to break free from their atoms.

**Figure 3**

1. **Electric Field:** The PV cell has an electric field created by the presence of positively and negatively charged layers within the material. This electric field helps separate the excited electrons from the atoms.
2. **Current Generation:** The separated electrons are collected by conductive metal contacts on the top and bottom of the PV cell. This flow of electrons creates a direct current (DC) that can be used as electricity.

****

1. **Conversion to Alternating Current (AC):** The DC electricity generated by the solar panels is then converted to alternating current (AC) using an inverter. AC electricity is the standard form of electricity used in most electrical systems, as for such the figure 4.

**Figure 4**

Once converted to AC, the electricity can be used to power various electrical devices, appliances, and homes or can be fed into the electrical grid to supply electricity to the wider community.

**2.2 Equations of Performance**

* **Solar Irradiance (G):** Solar irradiance represents the amount of solar energy received per unit area at a given location and time. It is typically measured in watts per square meter (W/m²). The equation for solar irradiance can be written as:

G is the solar irradiance

G₀ is the solar constant (approx. 1361 W/m²)

θ is the angle of incidence of sunlight on the surface

AM is the air mass factor (represents the path length of sunlight through the Earth's atmosphere)

*G = G₀ × cos(θ) × AM*

* **Incident Solar Power (P):** The incident solar power is the total amount of solar energy received by the solar panel over a given time period. It is calculated by multiplying the solar irradiance (G) by the area of the solar panel (A):

P is the incident solar power

G is the solar irradiance

A is the area of the solar panel

*P = G × A*

* **Efficiency of the Solar Panel (η):** The efficiency of the solar panel represents the ratio of electrical power output to the incident solar power. It takes into account losses due to various factors such as reflection, temperature, and electrical conversion losses

η is the efficiency of the solar panel

Pout is the electrical power output of the solar panel

Pin is the incident solar power

*η = (Pout / Pin) × 100%*

* **Electrical Power Output (Pout):** The electrical power output is the amount of usable electrical energy generated by the solar panel. It can be calculated by multiplying the incident solar power (P) by the efficiency (η):

Pout is the electrical power output

η is the efficiency of the solar panel

Pin is the incident solar power

*Pout = η × Pin*

* **Operating Cell Temperature (Tc):** The operating cell temperature represents the temperature of the solar panel during operation, taking into account factors such as ambient temperature, solar irradiance, and heat dissipation. It is typically higher than the ambient temperature and affects the electrical performance of the solar panel. The equation for calculating the operating cell temperature is:

Tc is the operating cell temperature

Ta is the ambient temperature

NOCT is the nominal operating cell temperature (provided by the manufacturer)

G is the solar irradiance

G₀ is the solar constant

*Tc = Ta + (NOCT - 20) × (G / G₀)*

* **Emissivity (ε):** Emissivity is a measure of a material's ability to emit thermal radiation. It affects the thermal balance of the solar panel and its temperature. The equation for calculating the net thermal radiation from a solar panel is:

Qrad is the net thermal radiation

ε is the emissivity

σ is the Stefan-Boltzmann constant (approx. 5.67 × 108 W/(m²·K⁴))

A is the surface area of the solar panel


T is the temperature of the solar panel

Ta is the ambient temperature

Qrad = ε × σ × A × (T4 – Ta4)

The power equation can be shown to be:

***Pexpected = (G₀ × cos(θ) × AM × A × η) × (1 + TC × (Tc - Tref))***



**Figure 5-Code 1-The power is calculated for each combination of incident angle and temperature using the provided formula.**

% Solar panel parameters

panelEfficiency = 0.15; % Efficiency of the solar panel

panelArea = 1; % Area of the solar panel in square meters

% Simulation parameters

temperatureRange = 20:5:60; % Range of temperature values to simulate (in degrees Celsius)

incidentAngleRange = 0:5:90; % Range of incident angle values to simulate (in degrees)

% Calculate power output for each combination of temperature and incident angle

powerOutput = zeros(length(temperatureRange), length(incidentAngleRange));

for i = 1:length(temperatureRange)

for j = 1:length(incidentAngleRange)

temperature = temperatureRange(i);

incidentAngle = incidentAngleRange(j);

% Calculate power output based on temperature and incident angle

powerOutput(i, j) = calculatePowerOutput(temperature, incidentAngle, panelEfficiency, panelArea);

end

end

% Create surface plot

figure;

surf(incidentAngleRange, temperatureRange, powerOutput);

% Customize the plot

xlabel('Incident Angle (degrees)');

ylabel('Temperature (\circC)');

zlabel('Power Output (W)');

title('Solar Panel Power Output');

colorbar; % Add a colorbar

% Helper function to calculate power output

function power = calculatePowerOutput(temperature, incidentAngle, efficiency, area)

% Assuming a simplified power calculation based on temperature and incident angle

power = efficiency \* area \* (1 - 0.005 \* (temperature - 25)) \* cosd(incidentAngle);

end


* 1. **Simulation**


To evaluate the performance of solar plants accurately, it is crucial to assess the power output and compare it against the theoretical power potential. This scientific study aims to investigate and analyze the disparities between the real and theoretical powers of a solar plant, shedding light on the factors that influence the efficiency and performance of solar power generation.

* ***Theoretical Power Calculation:***


THE SOLAR ANGLES

The solar panel’s output efficiency at max is ~22% and it heavily depends upon various internal and external factors. To begin with, solar angles are one of the crucial external factors to be considered while installing the PV panel on any roof. different types of solar angles and their methods of calculations are stated below:

* Azimuth angle:


it is calculated by measuring the angle between North 0 and the altitude angle. Besides, the altitude angle [a] is nothing but the angular elevation of the object above the observer’s horizon (**Figure 6-a**).


**Figure 6-a**

* Zenith angle:

the zenith angle becomes an angle between the zenith and the Sun. It works complementary with the elevation angle, in which angular motion is calculated between the horizon and the Sun. Zenith angle can be calculated as (**Figure 6-b**):

**Figure 6-b**





**Figure 6-b’**: The simulation of the given zenith formula


# Hour angle:

# 


The hour angle converts the local solar time into the amount of radians the sun moves across the sky (**Figure 6-c**). Note that, by convention, the hour angle is zero at solar noon, and, since the Earth rotates 2π/24 rad per hour, the hour angle ω can be simply calculated as follows:

**Figure 6-c**


***ω =π/12\* (t − 12)***

For Example:

* Declination angle




It is the angle made between the ray of the Sun, extended to the center of the Earth, and the equatorial plane of the Earth (**Figure 6-d**).

Whenever the rays of Sun reaches to the center of the Earth via Northern hemisphere, the declination angle becomes positive and whenever it reaches from the Southern hemisphere, it becomes negative.


**Figure 6-d**

the solar declination angle varies from -23.5 < d <23.5 degrees as pinpointed in **Figure 6-e.**

**Figure 6-e**





* Altitude angle




The solar altitude angle varies because of the three main factors which are, the time of the day, the time of the year, and the latitude of the Earth respectively (**Figure 6-f)**.

**Figure6-f**

The altitude angle can be calculated as



* Incidence angle

Finally, with respect to solar energy systems: the angle of the sun’s ray renders a line perpendicular to the earth; for example, the earth directly facing the sun has an angle of zero incidence, and the surface parallel to the sun (**Figure 6-g**)

**Figure 6-g**

*The MATLAB code provided allows you to simulate and visualize the variation of expected power from solar panels throughout the day. The code takes inputs such as the number of solar panels, their area,dates, and corresponding temperatures.*

function solarPlantGUI()

% Create a figure and GUI components

fig = figure('Name', 'Solar Plant Power Estimation', 'NumberTitle', 'off', 'Position', [200, 200, 800, 600]);

% Create input labels and fields

uicontrol('Style', 'text', 'String', 'Temperature (°C):', 'Position', [50, 500, 150, 20]);

temperatureEdit = uicontrol('Style', 'edit', 'Position', [200, 500, 100, 20]);

uicontrol('Style', 'text', 'String', 'Azimuthal Angle (°):', 'Position', [50, 450, 150, 20]);

azimuthalEdit = uicontrol('Style', 'edit', 'Position', [200, 450, 100, 20]);

uicontrol('Style', 'text', 'String', 'Inclination Angle (°):', 'Position', [50, 400, 150, 20]);

inclinationEdit = uicontrol('Style', 'edit', 'Position', [200, 400, 100, 20]);

uicontrol('Style', 'text', 'String', 'Longitude:', 'Position', [50, 350, 150, 20]);

longitudeEdit = uicontrol('Style', 'edit', 'Position', [200, 350, 100, 20]);

uicontrol('Style', 'text', 'String', 'Latitude:', 'Position', [50, 300, 150, 20]);

latitudeEdit = uicontrol('Style', 'edit', 'Position', [200, 300, 100, 20]);

uicontrol('Style', 'text', 'String', 'Number of Panels:', 'Position', [50, 250, 150, 20]);

numPanelsEdit = uicontrol('Style', 'edit', 'Position', [200, 250, 100, 20]);

uicontrol('Style', 'text', 'String', 'Panel Efficiency(%):', 'Position', [50, 200, 150, 20]);

efficiencyEdit = uicontrol('Style', 'edit', 'Position', [200, 200, 100, 20]);

uicontrol('Style', 'text', 'String', 'Panel Power (W):', 'Position', [50, 150, 150, 20]);

powerEdit = uicontrol('Style', 'edit', 'Position', [200, 150, 100, 20]);

uicontrol('Style', 'text', 'String', 'Panel Area (m^2):', 'Position', [50, 100, 150, 20]);

areaEdit = uicontrol('Style', 'edit', 'Position', [200, 100, 100, 20]);

% Create a submit button

submitButton = uicontrol('Style', 'pushbutton', 'String', 'Submit', 'Position', [50, 20, 100, 30]);

set(submitButton, 'Callback', @calculatePower);

% Callback function to calculate and plot power

function calculatePower(~, ~)

function x=HourAngle(hour)

x=-15 \*(12 - hour);

end

function x=DeclinationAngle(dayOfYear)

x= -23.45 \* cos((dayOfYear + 10) \* (360/365) \* deg2rad);

end

function x=ZenithAngle(dayOfYear,hour)

x=acosd(sind(latitude)\*sind(DeclinationAngle(dayOfYear))+ cosd(DeclinationAngle(dayOfYear))\*cosd(latitude)\*cosd(HourAngle(hour)));

end

function x=SolarAltitude(dayOfYear,SolarHour)


x=(asind(sind(DeclinationAngle(dayOfYear)) \*sind(latitude) + cosd(latitude)\*cosd(DeclinationAngle(dayOfYear))\*cosd(HourAngle(SolarHour))));

end

function x=IncidentAngle(hour,dayOfYear)

x= acosd(sind(latitude)\*sind(DeclinationAngle(dayOfYear))\*cosd(inclinationAngle)-cosd(latitude)\*sind(DeclinationAngle(dayOfYear))\*sind(inclinationAngle)\*cosd(azimuthalAngle)+cosd(latitude)\*cosd(DeclinationAngle(dayOfYear))\*cosd(hour)\*cosd(inclinationAngle)+cosd(DeclinationAngle(dayOfYear))\*sind(hour)\*sind(inclinationAngle)\*sind(azimuthalAngle)+sind(latitude)\*cosd(DeclinationAngle(dayOfYear))\*cosd(hour)\*sind(inclinationAngle)\*cosd(azimuthalAngle));

end

*It calculates the inclination angle theta and expected power at each time sample for each date using the provided formula. The inclination angle theta is determined based on the latitude, date, and time, while the expected power considers factors such as the solar constant, air mass, efficiency of the solar panel, temperature coefficient, and reference temperature. The power curves are then plotted, with each date represented by a different curve. The x-axis represents time in hours, and the y-axis represents the total expected power. This plot helps visualize the daily fluctuations in power output due to the changing inclination angle throughout the day.*

% Get input values

temperature = str2double(get(temperatureEdit, 'String'));

azimuthalAngle = str2double(get(azimuthalEdit, 'String'));

inclinationAngle = str2double(get(inclinationEdit, 'String'));

longitude = str2double(get(longitudeEdit, 'String'));

latitude = str2double(get(latitudeEdit, 'String'));

numPanels = str2double(get(numPanelsEdit, 'String'));

efficiency = str2double(get(efficiencyEdit, 'String'));

power = str2double(get(powerEdit, 'String'));

area = str2double(get(areaEdit, 'String'));

% Constants and parameters

G0 = 1361; % Solar constant (W/m^2)

AM = 1.5; % Air Mass factor

eta = efficiency/100; % Panel efficiency

TC = 0.005; % Temperature coefficient (%/°C)

Tref = 25; % Reference temperature (°C)

deg2rad = pi/180; %Convertion to degrees

DayOfYear = 1:365;

HoursOfDay = 1:24;

%Pexpected = (G0 \* cosd(theta)) \* AM \* panelArea \* eta \* (1 + TC \* (temperature - Tref));

figure;

[X,Y]=meshgrid(DayOfYear,HoursOfDay);

for i=1:24

for j=1:365

power(i,j)=G0\*cosd(IncidentAngle(i,j))\*AM\*numPanels\*area\*eta\*(1+TC\*(temperature-Tref));

end

end

surf(X, Y, power);

% Customize the plot

xlabel('Time (hours)');

ylabel('Day Of Year');

zlabel('Power(kw)');

title('Variation of Power');

colorbar; % Add a colorbar

colormap jet;


end

*By incorporating latitude and indirectly considering longitude through the local solar time, we were able to estimate the inclination angle theta, which represents the incident angle of sunlight. This allowed us to simulate and visualize the variation of expected power from solar panels throughout the day based on the changing angles of sunlight incidence.*



*The analogy illustrates how latitude and longitude coordinates, along with date and time, play a crucial role in solar energy calculations by determining the angles at which sunlight strikes a surface, thus impacting the efficiency and output of solar energy systems.*

*The simulated data consists of 22 PV cells each with the following specs* ***assumed efficiency of 20%***

***(Figure 7-a)***


**

**Figure 7-a:** PV specs


******


**Figure 7-b:** Input Parameters

* ***Data Collection:*** *The actual collected data is gathered by the adequate means into several excel sheets and exported to matlab and then resulting in the following:*




**Fig 8-a: Excel File with the collected data**






**Fig 8-b: Code2-The Power Production of the Battery, Inverter, and Solar**


**In 21-12-2022**



**Fig 8-b’: Code2-The Power Production of the Battery, Inverter, and Solar in 21-6-2022**




**Fig 8-c: Code2-The Power Production of the Battery, Inverter, and Solar in 21-9-2022**



**Fig 8-d: Code2-The Power Production of the Battery, Inverter, and Solar in 21-3-2022**

* ***Comparative Analysis:***

*The comparative analysis consists of formulating the maximum points of the obtained power curves, and thus obtain the maximal power production:*



**Fig 9: Comparison between real and theoretical Power Curve**



* ***Efficiency Assessment:***


*Calculating the difference between the* ***simulated power*** *and the* ***obtained maximal power*** *of the plants and dividing it by the real power results in the* ***yield coefficient****. The corrected efficiency assumed above is thus 20% \* the yield value.*

**3.1 Concept**

The wind power is the conversion of wind energy into useful form of energy such as using wind turbines to make electrical power. Wind power is the most efficient technology to produce energy in a safe and environmentally sustainable manner: it is zero emissions, local, inexhaustible and reduces the use of fossil fuels. It’s a rapidly growing source of renewable electricity worldwide.

***Wind Turbine:***

A Wind Turbine is a rotary mechanical device that collect and convert the kinetic energy that wind produces into electricity to help power the grid. There are primarily two types of wind turbines which are based on the axis about which the turbine rotates.

**** The major visible components of a utility-scale wind turbine **(Figure 8-a)** are a rotor, nacelle and tower. Along with the hub, wind energy generator, gearbox and yaw motor make up the main components of a wind turbine.

**The rotor** is the rotating part of a turbine; it consists of (mostly) three blades and the central part that the blades are attached to, the hub. Blades are not solid; they are hollow and are made of composite material to be light and strong. The blades have the form of an air foil (same as the wings of an airplane) to be aerodynamic.

**The nacelle** is housing on top of the tower that accommodates all the components that need to be on a turbine top. There are quite a number of components for the proper and healthy operation of a complicated electromechanical system that a turbine is.

**Figure 10-a: Wind Turbine Components**


**The gearbox** is a vital component of wind turbines; it resides in the nacelle. A gearbox increases the main shaft speed from around 12–25 rpm\* (for most of today’s turbines) to a speed suitable for its generator.

All new turbines are equipped with pitch control, which implies that their blades’ pitch angle can be adjusted so that the power output from a turbine is maximized at all times, while it does not overload the generator and mechanical structures of the blades, tower, and the rotor shaft.


***Wind Resources:***

The variability of wind resources is a fundamental characteristic that shapes the landscape of renewable energy generation. Wind resources exhibit natural fluctuations in speed and direction, presenting both challenges and opportunities for harnessing wind power. The variability of wind resources is influenced by factors such as local topography, weather patterns, and seasonal changes. This inherent variability necessitates careful planning and efficient utilization of wind energy. However, it also underscores the importance of advanced technologies and systems, such as wind forecasting, grid integration, and energy storage, to effectively manage and maximize the potential of this renewable resource.

***Wind Speed and Power Output:***

The power output of a wind turbine is directly related to the wind speed. Turbines are designed to operate within a specific range of wind speeds. The limits of the range are known as the cut-in speed and cut-out speed. The cut-in speed is the point at which the wind turbine is able to generate power. Between the cut-in speed and the rated speed, where the maximum output is reached, the power output will increase cubically with wind speed. The cut-out speed is the point at which the turbine must be shut down to avoid damage to the equipment. The cut-in and cut-out speeds are related to the turbine design and size and are decided on prior to construction. The expected shape of the power curve is shown in **(Figure 8-b)**

**Figure 10-b**

***Grid Integration:***

Wind farms are typically connected to the electrical grid to distribute the generated electricity. Grid integration involves managing the variability and intermittency of wind power, as wind speed is not constant. Grid operators utilize forecasting, energy storage systems, and flexible grid management techniques to ensure the reliable and stable integration of wind energy into the grid. A simplified representation of the integration is given in **(Figure 8-c)**

**Fig 10-c: Grid Integration**

**3.2 Equations of Performance**

* *Power Coefficient:*

The performance of wind turbines is typically described using several key parameters:

* ***Tip Speed Ratio (λ):*** The tip speed ratio is defined as the ratio of the tangential speed of the rotor blade tip to the wind speed. It is calculated using the equation:

λ = (ω \* R) / V

λ is the tip speed ratio

ω is the angular velocity of the rotor

R is the radius of the rotor

V is the wind speed

* ***Pitch angle (θ):*** The pitch angle (θ) of a wind turbine refers to the angle at which the rotor blades are set with respect to the incoming wind. The pitch angle is adjustable and is used to control the aerodynamic performance and power output of the turbine.
* ***Azimuthal angle (φ):*** The azimuthal angle is the angle that represents the horizontal orientation or position of the wind turbine rotor with respect to a reference direction. It is usually measured in degrees or radians

The specific equation for determining the pitch angle depends on the design and control strategy of the wind turbine.

**Power Coefficient (Cp):** the power coefficient represents the efficiency of a wind turbine in extracting power from the wind. It’s calculated using the following equation:

Cp = (Pout / (0.5 \* ρ \* A \* V^3))

Cp is the power coefficient

P is the power extracted by the turbine (output power)

ρ is the air density

A is the swept area of the turbine rotor

V is the wind speed

There are different equations to calculate Cp based on the tip speed ratio and pitch angle, depending on the specific wind turbine design and characteristics

**Betz Limit Equation:**

The Betz limit equation represents the maximum power coefficient that can be achieved for an ideal wind turbine:

**Cp = 16/27 \* (1 - sqrt(1 - (λ/8)^2))**

According to Betz's law, the maximum power coefficient is approximately 0.59 (or 59%). This limit is derived from theoretical considerations and represents the maximum amount of power that can be extracted from the wind.

**Glauert's Correction:**

Glauert's correction is applied to account for the non-linearity of the power coefficient at high tip speed ratios. It is typically used for horizontal axis wind turbines:

Cp = (0.5 \* ρ \* A \* (1 - a)^3 \* (σ \* Cl \* sin(θ) - Cd \* cos(θ))) / (λ^2)

ρ is the air density,

A is the swept area of the rotor,

a is the axial induction factor (related to the wind speed reduction due to the rotor),

σ is the solidity of the rotor (ratio of blade area to rotor area),

Cl is the lift coefficient of the blade,

Cd is the drag coefficient of the blade.

**Blade Element Momentum Theory (BEM):**

The Blade Element Momentum (BEM) theory is a more advanced approach that divides the rotor into small segments and calculates the power coefficient based on the local conditions at each segment.

**Cp = (8 \* a \* (1 - a)^2 \* sin(θ)) / (λ^2 \* cos(θ))**

**\***Note that all these equations are approximations to the output power efficiency.

**3.3 Simulation**

*In the following code we’ll determine the power coefficient in terms of the tip speed ratio considering different pitch angles*

rho = 1.225; % Air density [kg/m^3]

A = 1; % Reference area [m^2]

a = 0.3; % Axial induction factor

sigma = 0.95; % Blade solidity

Cl = 1.5; % Lift coefficient

Cd = 0.08; % Drag coefficient

lambda = linspace(1, 10, 100); % Tip speed ratio

% Constant theta values

theta = [0, 15, 30, 45, 60,90];

% Calculate Cp for each theta

Cp = zeros(length(theta), length(lambda));

for i = 1:length(theta)

Cp(i, :) = (0.5 \* rho \* A \* (1 - a)^3 \* (sigma \* Cl \* sin(deg2rad(theta(i))) - Cd \* cos(deg2rad(theta(i))))) ./ (lambda.^2); %Using Glauret’s Correction equation

end

% Plot graph

figure;

plot(lambda, Cp');

xlabel('\lambda (Tip Speed Ratio)');

ylabel('Cp');

title('Cp vs. \lambda for different \theta');

legend('\theta = 0', '\theta = 15', '\theta = 30', '\theta = 45', '\theta = 60','\theta=90', 'Location', 'best');

grid

(THE Graph is shown in Fig 11-a)

% Define the range of lambda values

lambda = 1:0.025:10;

% Define the constant values of the pitch angle

theta\_values = [15,30,45,90];

% Plot Cp vs. lambda for different values

figure;

hold on;

Output\_Power=zeros(size(lambda));

for theta = theta\_values

% Calculate Cp for each value of lambda using BEM theory

Cp = (8 \* theta \* (1 - theta)^2 \* sin(theta)) ./ (lambda.^2 \* cos(theta));

plot(lambda, Cp, 'LineWidth', 2);

end

hold off;

% Set plot labels and title

xlabel('(Tip Speed Ratio)');

ylabel('Cp (Power Coefficient)');

title('Power Coefficient vs. Tip Speed Ratio for Different Pitch Angles');

% Add a legend

legend(string(theta\_values), 'Location', 'best');

grid

(The graph is shown in Fig 11-b)



 Simulation using BEM theory equation: Using Glauert’s correction equation:

Fig 11-b

**Fig 11-a**

Analysis:

As seen in the preceding figures When the tip speed ratio is low, the wind turbine operates at a relatively low rotational speed compared to the wind speed. In this regime, the aerodynamic forces on the blades are typically low, resulting in a lower power coefficient. As the tip speed ratio increases, the blades rotate faster relative to the wind speed. This allows the turbine to extract more energy from the wind. However, operating at very high tip speed ratios can lead to diminishing returns, as the increased rotational speed may introduce aerodynamic inefficiencies and mechanical stresses that limit further power extraction.

Also, the pitch angle plays a significant role in determining the performance of a wind turbine. Wind turbines are designed to operate at an optimal pitch angle that maximizes their power output for a given wind speed. This angle is typically determined through extensive design and testing processes. However, operating with a pitch angle different from this optimal angle, the blades will be unable to effectively capture the available wind energy.

* *Output Power:*
* **Wind Power and Power Curve:**

The theoretical wind power available from the mass flow rate of air through the turbine blades swept area is obtained by

**Pw=** **ρAv3**  if vcut-in ≤v≤vrated

**ρ** is the air density

A is the turbine rotor area in m2

V is the wind speed

**0** if v<vcut-in or v>vcut-out

**Prated**  if v rated≤v≤vcut-out

* In this section we’ll compare real data of output power of a wind turbine with the theoretical power curve:

data1=xlsread('C:\Users\CompuTop\OneDrive\Documents\Book3.xlsx','Sheet1','B1:D488');

% we have determined the power output and the wind speed for 48 hours

% with 10 mins time interval with the wind speed

wind\_speed=data1(:,2);

realpowerdata=data1(:,1);

%defining constants

rho=1.225; %air density

A=24; %area of the blade rotor in m^2

cutinspeed=3; %wind speed at which wind turbine starts generating power in m/s

cutoutspeed=20; %wind speed at which wind turbine stops generating power in m/s

ratedspeed=13; %rated wind speed

ratedpower=3600; %these constants are deduced from the real data

theoretical\_power=zeros(size(wind\_speed));

for i=1:length(theoretical\_power)

if wind\_speed(i)<cutinspeed || wind\_speed(i)>cutoutspeed

theoretical\_power(i)=0;

elseif wind\_speed(i)>=cutinspeed && wind\_speed(i)<=ratedspeed

theoretical\_power(i) = (wind\_speed(i) - cutinspeed) / (ratedspeed - cutinspeed) \* ratedpower;

else

theoretical\_power(i)=ratedpower;

end

end

%we have made a polynomial of degree 3 regression of the theoretical power

p=polyfit(wind\_speed,theoretical,3);

theoretical=polyval(p,wind\_speed);

plot(wind\_speed,theoretical,'b-');

hold on;

plot(wind\_speed,realpowerdata,'r-');

xlabel('Wind Speed in m/s');


ylabel('Output Power');

title('Comparison Between the real output power and the theoretical one');

legend('theoretical data','real power data');

hold off;

grid on;



**Fig 10: Wind Power Curve**

The chosen regression polynomial for the theoretical power is close to the real power curve

* **Time series analysis:**

Time series analysis of a wind turbine refers to the process of analyzing and modeling the data collected from a wind turbine over time.

1. Hourly analysis:

[~,time1]=xlsread('C:\Users\CompuTop\OneDrive\Documents\Book2.xlsx','Sheet1','A2:A50531');


% We have loaded into the vector time text data which represent the date time

Outputpower=xlsread('C:\Users\CompuTop\OneDrive\Documents\Book2.xlsx','Sheet1','B2:B50531');

plot(datenum(time1),outputpower);

xlabel('date');

ylabel('OutputPower');



**Fig 11-a: Hourly Analysis During 2018**

It is not convenient to see an hourly plot like this. Instead, we can group the data frame by hours (hour 0 to 24) then take average of active power.

%time series analysis

[~,time1]=xlsread('C:\Users\CompuTop\OneDrive\Documents\Book2.xlsx','Sheet1','A2:A50531');

% We have loaded into the vector time1 text data type which represent the

%Date time

%We want to generate on average the output power at each hour of the day

outputpower=xlsread('C:\Users\CompuTop\OneDrive\Documents\Book2.xlsx','Sheet1','B2:B50531');

%We've loaded the corresponding output power at each time

time1 = datetime(time1, 'InputFormat', 'dd MM yyyy HH:mm');

hours=zeros(24,1);

temp=hour(time1);

for i=1:6:(size(temp)/6)

temp1=0;

for j=(i - 1) \* 6 + 1:(i - 1) \* 6 + 6

temp1=temp1+outputpower(j);

end

hours(1+temp(i))=hours(1+temp(i))+temp1/6;

end


hours=hours/365\*6;

vect=0:1:23;

plot(vect,hours,'b-');

xlabel('hours');

ylabel('Average output Power per hour');

 grid on;

**Fig 11-b: Average Output Power during 24hours**

Power drop during the noon-hours. Peak values afternoon and during the night. This can be due to the wind speed variations which is influenced by many factors, including the diurnal heating of the Earth's surface, which leads to a decrease in temperature gradients and, consequently, weaker winds. Additionally, atmospheric stability during the day can suppress vertical mixing and reduce wind speeds near the ground. Lower wind speeds directly impact the output power of a wind turbine since the power generated is proportional to the cube of the wind speed. Also, Turbulence and Wind Shear: During noon, the atmospheric boundary layer (the layer of the atmosphere closest to the Earth's surface) tends to be more stable, leading to reduced turbulence and wind shear. Wind shear refers to the change in wind speed and direction with height.

1. Monthly analysis:

[~,time1]=xlsread('C:\Users\CompuTop\OneDrive\Documents\Book2.xlsx','Sheet1','A2:A50531');

outputpower=xlsread('C:\Users\CompuTop\OneDrive\Documents\Book2.xlsx','Sheet1','B2:B50531');

time1 = datetime(time1, 'InputFormat', 'dd MM yyyy HH:mm');

months=zeros(12,1);

temp=month(time1);

for i=1:size(temp)

months(temp(i))=months(temp(i))+outputpower(i);

end

months=months/(30\*24\*6);

vect = 1:1:12;


plot(vect,months)

xlabel('Months');

ylabel('Average output Power');

title('Average Output Power during each month of the year');

grid on;



**Fig 11-c: Average Output Power during each month**

Power drop during July. Peak values during March, August and October. This can be attributed to various factors related to wind patterns, weather conditions, and environmental factors. Wind patterns can exhibit seasonal variations due to changes in atmospheric conditions. In many regions, there are certain times of the year when wind speeds are more favorable for wind power generation. During Spring or Fall, transitional periods between seasons, there can be increased variability in atmospheric conditions, leading to more frequent and stronger wind patterns. These periods often experience more frequent weather systems, frontal boundaries, and pressure gradients, resulting in higher wind speeds and, subsequently, higher power output. Conversely, during summer, particularly in July, there can be a shift in wind patterns. In some regions, the presence of high-pressure systems or stable atmospheric conditions during this time can lead to lower wind speeds and reduced power output from wind turbines.

**Conclusion**

In conclusion, this report has shed light on the transformative power of renewable resources in addressing the analysis considering various environmental and technical factors. By harnessing the renewable resources, we can transcend the limitations of traditional energy infrastructure and bring electricity to underserved areas. This output power has proven to be a game-changer, offering a sustainable and decentralized solution to power generation.

The variability of these resources during time and the losses due to the limitations of the architecture of traditional grids sheds the light on the importance to have an algorithm/ device that optimizes the power delivered and here comes the role of a smart grid. with the advent of the smart grid, we have witnessed a paradigm shift in our ability to accommodate and optimize the variable nature of renewable energy. Through advanced monitoring, forecasting, and control mechanisms, the smart grid seamlessly integrates with wind energy systems, enabling real-time adjustments and adaptive strategies. This intelligent coordination allows for efficient balancing of the grid by dynamically allocating power resources as per demand and grid conditions. By embracing the potential of the smart grid, we can leverage the abundant and clean energy, paving the way for a brighter and more sustainable future for generations to come.

1. **References:**

<https://www.energy.gov/eere/wind/wind-energy-basics>

<https://theroundup.org/wind-turbine-power-curve/>

<https://ieeexplore.ieee.org/document/6894235?denied=>

<https://energysavingtrust.org.uk/advice/solar-panels/>

<https://www.siemens.com/global/en/products/energy/grid-software/operation/grid-control.html?acz=1&gclid=Cj0KCQjwwISlBhD6ARIsAESAmp6YhjIoRDhAXcqHPvIM4wJrlVLaoxi8arzMJmPJ3QTE-lXrcBqhWWIaAsL4EALw_wcB>

<https://www.nrel.gov/solar/>

<https://www.tntech.edu/engineering/research/cesr/smartgrid/smart-grid-lab.php>